

MIDDLE EAST TECHNICAL UNIVERSITY

DEPARTMENT OF ELECTRICAL AND ELECTRONICS ENGINEERING

EE464 Simulation Project-2 Report

Isolated Converters & Controller Design

19/04/2018

Hakan Saraç - 2041838

Mahmut Enes Kara - 2030898

Cem Kavuncu - 2030963

Table of Contents

[1. Introduction](#_Toc494829768) 2

[2. Results](#_Toc494829775) 2

[3. Conclusion 25](#_Toc494829801)

1. **Introduction**

In this project, we are required to design an isolated DC-DC converter and a controller, respectively. For DC-DC converter, we are supposed to use the topology that we chose for our hardware project. Therefore, since we have chosen to use flyback converter for our hardware project, firstly we need to design a transformer for our flyback converter. Secondly, we are supposed to observe the voltage-current stress in the switches and decide to use any snubber. Also, we are objected to choose our components for our converter. Moreover, we are supposed to design a converter for our specifications in the hardware project and obtain its bode plot and transfer function. Lastly, we are supposed to design a Type-2 controller.

Our converter specifications are as follows.

|  |  |  |  |
| --- | --- | --- | --- |
| **Vin (Vdc)** | **Vout (Vdc)** | **Pout (W)** | **Topology** |
| 12 | 24 | 80 | Flyback |

1. **Results**

**Q1) Isolated Converter Simulation**

The given constraints of the Flyback converter is 80W of output power rating, input voltage of 24V and output voltage of 12V. To achieve that we have decided upon the following specifications for our converter. Calculation of values (Lm,C) and the choice of the elements are provided in the following sections.

**Table 1.1: Chosen element list**

|  |  |  |  |
| --- | --- | --- | --- |
|  | Value | Voltage Rating | Current Rating |
| C | 470µF | 50V | - |
| Lm [(core)](https://www.digikey.com/product-detail/en/epcos-tdk/B65887E0160A041/495-5332-ND/3914482) | 256µH | - | 8.33Aavg |
| [Mosfet](https://www.digikey.com/product-detail/en/on-semiconductor/FQPF22P10/FQPF22P10-ND/1055387) | - | 100V | 13.2A |
| [Diode](https://www.digikey.com/product-detail/en/vishay-semiconductor-diodes-division/VFT2045BP-M3-4W/VFT2045BP-M3-4W-ND/3102973) | - | 45V | 20A |

In the steady state under full load, we have designed our converter achieve CCM under full load. The switching frequency is chosen as 10kHz in order to achieve greater efficiency. Low switching frequency is compensated by using a bigger core and larger number of turns. Output capacitor is chosen large deliberately in order to achieve low voltage ripple at the output. Since the voltage ratings are low size of the capacitor is not a big issue in this converter. Moreover, there is no limitation in the size as well. The transformer ratio is chosen as N1/N2 = 2.



**Figure 1.1: Output voltage waveform at the steady state**

1. **Transformer design**

In this part, and most of the parts, the calculation is done using MATLAB. You can reach to the related m file in our Github repository.

Transformer is the key component in a flyback converter. It should be capable of storing and delivering enough energy to the output in a switching cycle. As the switching frequency increases Lm value can be reduced because the ripple current on the Lm is directly related to the switching frequency. Before starting to the transformer design, ripple of the current flowing through the Lm is assumed to have a ripple of 40%. Using this constraint following values are calculated. Moreover, duty cycle is chosen as 0.4, which is a reasonable duty ratio.

Note that, as duty cycle gets too close to 0 or 1, operation of any converter is affected badly since the inductor is charged or discharged for a very short amount of time, proper operation may not be achievable.

To achieve 288µH, a core with a high AL value should be chosen. Core should be gapped in order to store more energy. To achieve the given specifications, we have chosen the core with the chosen specifications. To reach to the datasheet, you can click [here](https://www.digikey.com/product-detail/en/epcos-tdk/B65887E0160A041/495-5332-ND/3914482).

**Table 2: Specifications of the transformer core**

|  |  |
| --- | --- |
| Flux Density | 0.49T |
| Effective Core Area (Ae) | 200mm2 |
| Effective Length (le) | 70mm |
| Inductance Factor (Al) | 160nH |
| Effective Permeability (µe) | 45 |
| Effective Magnetic Volume (Ve) | 14000mm³ |
| Material | N41 |

Number of turns required for to reach to the calculated Lm value:

Based on this calculation, N1 chosen as 40 turns. The current flowing in the primary side is calculated as half of the load current (since N1/N2 = 2 chosen) that is 3.33A. Referring to the table in this [link](https://www.powerstream.com/Wire_Size.htm), AWG 16 cable can carry 3.7A of current which has 1.29mm of diameter. The window area of the core is given as 20.8\*7mm2. Fill factor of the core is:

With the addition of the secondary side cables, FF value will be around 0.7, which is achievable.

The core also should not get saturated the maximum value of the Lm value. Peak value of the flux density of the is calculated as:

From the datasheet, it can be seen that the loss coefficient at 0.3T and 10khz is around 100kW/m3.

1. DCM occurs when ILmmin reaches zero. Assuming current ripple on the Lm is constant,

then ILm=1.667A at the boundary of the DCM. Also, we know that Is=D\*ILm = 0.4\*1.667 = 0.667A. Therefore when the load current goes below N1/N2\*Is = 2\*0.667 = 1.333A, the converter goes into the DCM.


Due to the energy stored in the leakage inductance, when the switch goes off, large di/dt rate causes very high voltage peaks. To overcome this problem, the transformer can be designed to have smallest leakage inductance, or the switch be chosen very large to suppress the extra voltage stress. We have modeled our leakage inductance as 2.3µH on the primary side. The voltage across the switch element is shown in Figure 1.2. Note that in order to model the chosen switching element, Rdson value of the mosfet is set, and a parallel capacitance of 930pF is put across the mosfet for the Cgs capacitance modeling.

The formulas used in this part is taken from [here](https://www.fairchildsemi.com/application-notes/AN/AN-4147.pdf).



**Figure 1.2: Voltage across the switch in the steady state**


During the turning off, the voltage across the switch reaches up to 4.6kV. Choosing a switching element at that rates is not a viable solution for such an low powered application. Therefore, we have designed an RCD snubber circuit in order to reduce the voltage stress across the switch. The schematic of the RCD snubber circuit and its connection to the flyback converter is given in Figure 1.3.



**Figure 1.3: Flyback converter with RCD snubber**[**(source)**](https://www.fairchildsemi.com/application-notes/AN/AN-4147.pdf)

To design the snubber, we have followed the steps provided in the application note of the ON Semiconductor. You can reach the application from [here.](https://www.fairchildsemi.com/application-notes/AN/AN-4147.pdf)

Before starting the calculations, we have given some predetermined values to the Csn and Rsn to determine Vsn value. The waveform of Vsn is shown in Figure 1.4.




**Figure 1.4: Vsn waveform**[**(source)**](https://www.fairchildsemi.com/application-notes/AN/AN-4147.pdf)


These values are found by trial and method and Csn =2µF Rsn=25Ω. After finding suitable values for Csn and Rsn in order to determine Vsn value, we have followed following steps. Note that peak value of the iD current (Figure 1.3) is also determined for this purpose.

Assuming 10% voltage ripple across the Csn capacitor;

When have simulated for Rsn = 93.44Ω and Csn = 10.7µF.



**Figure 1.5: Voltage across the Csn capacitor**



**Figure 1.6: Voltage across the switch element**

Using the designed RCD snubber circuit, it can be seen that the voltage stress across the switching element is reduced to 50V. Even though there is still some resonance, the high voltage peaks are eliminated.

1. **Efficiency**


The change in the load current changes the ILm value, which varies the core losses value as well. Using the created m file, the calculated values are as follows

**Table 1.3: Loss and Efficiency table.**


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Load** | **Bmean** | **Core loss** | **Total Switch loss** | **Diode loss** | **Copper loss** | **Efficiency** |
| 80W | 0.27T | 14W | 1.39W | 4.4W | 2.54W | 78% |
| 60W | 0.20T | 7W | 0.78W | 3.3W | 1.42W | 83% |
| 40W | 0.135T | 2.8W | 0.35W | 2.2W | 0.63W | 87% |
| 20W | 0.08T | 0.7W | 0.09W | 1.1W | 0.15W | 91% |
| 0W | 0T | 0W | 0.005W | 0W | 0W | 100% |

1. **Components**

The rating values of the component is provided in part a Table 1.1. The choice of these elements is made according to the simulation results. The waveforms of the mosfet and the diode are as follows.



**Figure 1.7: Mosfet current waveform**



**Figure 1.8: Diode voltage and current waveforms**

Mosfet current has a mean value of 4.55A with the addition of the losses, however its peak reaches 10.76A. During this peak value, mosfet can get heated up which can burn the device, therefore it should either be cooled down properly or chosen larger that peak value. In Figure 1.8, the maximum voltage across the mosfet is measured as around 60V.The datasheet of the chosen mosfet can be reached from [here](https://www.digikey.com/product-detail/en/on-semiconductor/FQPF22P10/FQPF22P10-ND/1055387).

Diode current swings between 20A and 0 and has a mean value of 6.8A. Moreover, maximum reverse voltage is around 24V. Considering these, we have chosen [this diode](https://www.digikey.com/product-detail/en/vishay-semiconductor-diodes-division/VFT2045BP-M3-4W/VFT2045BP-M3-4W-ND/3102973).

The capacitance value was calculated to get a output voltage ripple of 10%, which resulted in 222µF. To decrease the ripple further, we have chosen output capacitor as 470µF.

The rated values of the elements are provided in the Table 1.1 along with the links to their datasheets.


**2) Controller Design**

In this part, we designed a buck converter with input voltage of 24 V, output voltage of 12 V and power rating of 80 W, therefore same specifications is provided with the chosen Hardware Project.

**a)**

In this part, a buck converter transfer function is obtained analytically. In order to make the model realistic ESR values of both inductor and capacitor is added to converter schematic as seen in Figure xx. As marked in the schematic, there are two state variables in the buck converter namely inductor and capacitor current.

and Vo = C\*X where So, aim is finding A, B,C vectors.

 Figure xx: Realistic buck converter

*On State of buck converter*

As known, LCR circuit is connected to Vd through MOSFET in on state. Hence two mesh equations can be written such that one of them is covering outer mesh which consists of input voltage, inductor and load resistor and other one is covering capacitor and load resistor.

Kirchoff Voltage Law on outer mesh:

(1)

Kirchoff Voltage Law on small mesh:

(2)

From 2nd equation;

(3)

From 1st and 3rd equation;

(4)

Hence A1 and B1 matrices can be constructed as follows

Output voltage equation;

So;

*Off State of buck converter*

At off state, LCR circuit is short circuited through diode. Note that off state is exactly same with on state with Vd short circuited. So A2 = A1 and B2 = 0. Also output voltage equation is same which yields C2 = C1.

Resultant matrices;

A = A1 = A2 B= B1\*D C= C1= C2

As ESR of the inductor and capacitor is usually in mΩ range and minimum Rload is about 1.8Ω a reasonable assumption can be done with Rload >>rC,rL also Rload>>rC+rL. Resultant matrices can be constructed as follows;

*Obtaining Transfer Function*

From Mohan’s book at page 325 this transfer function formula can be seen;

C:\Users\St\Desktop\mohan tf.png

By substituting matrices found before it can be expressed as follows;

Taking inverse of middle matrices;

Hence;

Substituting numerical values; C =470 µF, L =1 mH, rC =10 mΩ, rL = 10 mΩ and R =1.8 Ω

Note that the terms results from rC and rL makes very small effect in denominator, but rC results a zero which may causes considerable differences at high frequencies. Bode plot of this transfer function is obtained using MATLAB, related result can be seen in Figure xx





Figure xx: Bode plot of analytically calculated transfer function

**b)**



**Figure 1:** The schematic circuit of the designed Buck Converter



**Figure 2:** The Bode plot of the simulated Buck Converter

We chose to use PSIM for simulating our converter design. We chose the capacitor value as 470uF and inductor value as 1mH. Also, we considered the equivalent series resistance of the capacitor and inductor as 0.01Ω.

As can be seen in both bode plot graphs, they are same noting that one of them is plotted to rad/s while other is plotted to Hz. As a consequence, it can be noted here that phase margin of the converter is about 20° and it should be improved by adding phase at the gain cross over frequency with the Type-2 controller in order to have more stable converter and better transient performance.

**c)**



**Figure 3:** The schematic circuit of the designed Buck Converter with Type-2 controller

In order to produce enough transient stability for our converter, we designed a Type-2 controller and chose the components of it. It can be seen as follows.

****

**Figure 4:** The schematic circuit of the Type-2 controller



**Figure 5:** The output voltage of the Buck Converter with Type-2 controller

We chose 2.2nF for the capacitor values, 10Ω for the first resistor and 50Ω for our second resistor. We considered the following equations in order to find a proper values for them.





We firstly decided the 10Ω value for the first resistor and calculate the gain with the following equation:



After that we found the gain, we calculated the capacitor values and the other resistor value, respectively. We tried them on the simulation and changed them with manually for the best operation.

**d)**



**Figure 6:** The change in the output voltage when the load is changed from half load to full load

****

**Figure 7:** The change in the output voltage when the supply voltage is decreased 10%

**e)**

When we changed the load or supply voltage, we observed some peak values in the output voltage. However, it fixed itself. When we increase the capacitor values in the controller circuit, we observed that firstly, the ripple of the output voltage is increasing and after that we increase the value to mF range and further, we also observe resonancy. However, when we decreased the capacitor value to pF range, we observed that no change occur for the peak value at the step change; however, ripple of output is decreased. For the increase in the first resistor value, we observed that the ripple at the output voltage is increased. Therefore, we chose small resistor value for this component.

1. **Conclusion**

In this project, we have examined different aspects of designing a power supply. In the first part design of a flyback converter is studied. There are several important points in designing of a flyback converter. One of them is the leakage inductance of the transformer causes overvoltages across the switching elements. This effect can be reduced with a better transformer design, however snubber design seems to be necessary to overcome this problem. The other one can be the design of the transformer. The core must be capable of carrying the load current without getting saturated and core loss must be high for the efficiency and cooling considerations.

In the second part, the design of a buck converter and its controller design is examined. The controllers are necessary for the power circuits because in the real life load current or the input voltage is not constant. We have used analog controller because they are simpler to implement and have faster response then the digital controllers. The transfer function of the buck converter is obtained including the parasitic resistances of the passive elements. Depending on this transfer function, bode plots are drawn. To improve the phase margin and reduce the steady state error, a type 2 controller is implemented which is a PI controller. Depending on the values of the resistances and the capacitances of the controller, pole locations can be set and desired bode plot can be obtained. By choosing these values properly, the converters stability can be increased, and the steady state error can be decreased.